Metadata-Version: 2.1
Name: maxcul
Version: 0.1.1
Summary: Access with Python MAX! Devices over a CUL Stick
Home-page: https://github.com/karlTGA/MaxCul-Python
Author: Markus Ullmann, Karl Wolffgang
Author-email: karlwolffgang@googlemail.com
License: BSD License
Platform: any
Classifier: Programming Language :: Python
Classifier: Development Status :: 4 - Beta
Classifier: Natural Language :: English
Classifier: Environment :: Console
Classifier: Intended Audience :: Developers
Classifier: License :: OSI Approved :: BSD License
Classifier: Operating System :: OS Independent
Classifier: Topic :: Software Development :: Libraries :: Python Modules
Classifier: Topic :: Home Automation
Provides-Extra: testing

# About MaxCul for Python

This Module is forked from this Project https://github.com/jokey2k/MoritzServer.
It can communicate over a serial connection and a cul stick with MAX! Devices build by eQ-3 http://www.eq-3.de/produkte/max.html.

The CUL (or CC1101 USB Lite) is a USB Stick, which sends and receive Packages in the 868Mhz frequency.
The FHEM community developed a open firmeware for the stick and so the MAX! protocol ist only one of many protocols you can use with this stick.
I build my own stick with this instruction: https://wiki.fhem.de/wiki/Selbstbau_CUL
But you can buy it for example here: http://www.busware.de/tiki-index.php?page=CUL

To install the dependecys use this command.
```
python setup.py install
```

After that you can start a test server with this command.
```
python bin/moritz-server.py --cul-path /dev/ttyUSB0
```
This open a small webserver with some tools to control your devices and see there states.



